{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["BOM_WFG100A_WFG100A_2025-11-18"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BOM_WFG100A_WFG100A_2025-11-18","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[]}
["No.","Quantity","Comment","Designator","Footprint","Value","Manufacturer Part","Manufacturer","Supplier Part","Supplier","备注"]
["1",20,"FC60PAD","A1,A2,A3,A4,A5,A6,A7,A8,A9,A10,A11,A12,A13,A14,A15,A16,A17,A18,A19,A20","FC60PAD","","","","","","此为焊盘，非物料。采购时直接忽略！！"]
["2",2,"1uF","C1,C4","C0603","1uF","0603B105K500NT","FH(风华)","C90540","LCSC","此为电池两端的电容，耐压值最低要选择35V以上的，推荐直接采用50V"]
["3",4,"10uF","C2,C3,C5,C6","C0805","10uF","0805X106K500NT","FH(风华)","C6117579","LCSC","此为电池两端的电容，耐压值最低要选择35V以上的，推荐直接采用50V"]
["4",26,"100nF","C7,C10,C13,C14,C19,C22,C23,C25,C26,C27,C28,C29,C33,C35,C37,C40,C41,C42,C44,C45,C46,C47,C48,C49,C51,C52","C0402","100nF","0402B104K500NT","FH(风华)","C110251","LCSC"]
["5",4,"22uF","C8,C9,C11,C12","C0805","22uF","0805X226M250NT","FH(风华)","C129303","LCSC","C11、C12是并联在10V电源两端，因此要选用16V的电容！！"]
["6",4,"10uF","C15,C16,C17,C18","C0603","10uF","0603X106M250NT","FH(风华)","C479655","LCSC"]
["7",4,"2.2uF","C20,C21,C34,C36","C0402","2.2uF","0402X225K160NT","FH(风华)","C501836","LCSC"]
["8",2,"4.7uF","C24,C43","C0402","4.7uF","0402X475K100NT","FH(风华)","C191541","LCSC"]
["9",2,"10nF","C30,C32","C0402","10nF","0402B103K500NT","FH(风华)","C1524","LCSC"]
["10",1,"470nF","C31","C0402","470nF","0402X474K100NT","FH(风华)","C967572","LCSC"]
["11",2,"10uF","C38,C39","C0402","10uF","0402X106M100NT","FH(风华)","C2846677","LCSC"]
["12",1,"1uF","C50","C0402","1uF","0402X105K160NT","FH(风华)","C167339","LCSC"]
["13",1,"SMAJ30CA","D1","DO-214AC_L4.3-W2.7-LS5.0-BI","","SMAJ30CA","宏迦橙","C19077548","LCSC"]
["14",1,"B5819W SL","D2","SOD-123_L2.7-W1.6-LS3.7-RD-1","","B5819W SL","CJ(江苏长电/长晶)","C8598","LCSC"]
["15",1,"USBLC6-2P6","D4","SOT-666-6_L1.6-W1.2-P0.50-LS1.6-BR","","USBLC6-2P6","ST(意法半导体)","C15999","LCSC"]
["16",1,"JK-nSMD050-30","F1","F1206","","JK-nSMD050-30","JK(金科)","C720075","LCSC"]
["17",2,"10uH","L1,L2","IND-SMD_L5.4-W5.2_FXL0530","10uH","FXL0530-100-M","cjiang(长江微电)","C177248","LCSC"]
["18",1,"BLM15PD121SN1D","L3","L0402","","BLM15PD121SN1D","muRata(村田)","C76891","LCSC"]
["19",1,"NCD0603W1","LED1","LED0603-RD","","NCD0603W1","国星光电","C84265","LCSC"]
["20",1,"NCD0603B1","LED2","LED0603-RD","","NCD0603B1","国星光电","C84266","LCSC"]
["21",1,"STM32H743VIT6","MUC1","LQFP-100_L14.0-W14.0-P0.50-LS16.0-BL","","STM32H743VIT6","ST(意法半导体)","C529058","LCSC","STM32主控淘宝翻新料的价格在20元左右，全新料在30元左右。"]
["22",1,"SS8050","Q1","SOT-23-3_L2.9-W1.3-P1.90-LS2.4-BR","","SS8050","CJ(江苏长电/长晶)","C2150","LCSC"]
["23",2,"1MΩ","R1,R3","R0402","1MΩ","0402WGF1004TCE","UNI-ROYAL(厚声)","C26083","LCSC"]
["24",2,"41.2kΩ","R2,R4","R0402","41.2kΩ","0402WGF4122TCE","UNI-ROYAL(厚声)","C26978","LCSC"]
["25",1,"7.68kΩ","R5","R0402","7.68kΩ","0402WGF7681TCE","UNI-ROYAL(厚声)","C25919","LCSC"]
["26",2,"51kΩ","R6,R8","R0402","51kΩ","0402WGF5102TCE","UNI-ROYAL(厚声)","C25794","LCSC"]
["27",1,"3.4kΩ","R7","R0402","3.4kΩ","0402WGF3401TCE","UNI-ROYAL(厚声)","C4940","LCSC"]
["28",2,"20Ω","R9,R10","R0402","20Ω","0402WGF200JTCE","UNI-ROYAL(厚声)","C25089","LCSC"]
["29",12,"100Ω","R11,R13,R32,R35,R36,R37,R38,R39,R40,R41,R42,R43","R0402","100Ω","0402WGF1000TCE","UNI-ROYAL(厚声)","C25076","LCSC"]
["30",16,"10kΩ","R12,R14,R15,R16,R22,R23,R24,R25,R29,R31,R44,R45,R46,R47,R48,R49","R0402","10kΩ","0402WGF1002TCE","UNI-ROYAL(厚声)","C25744","LCSC"]
["31",2,"75Ω","R17,R21","R0402","75Ω","0402WGF750JTCE","UNI-ROYAL(厚声)","C25133","LCSC"]
["32",4,"4.7kΩ","R18,R20,R33,R34","R0402","4.7kΩ","0402WGF4701TCE","UNI-ROYAL(厚声)","C25900","LCSC"]
["33",3,"1kΩ","R19,R26,R30","R0402","1kΩ","0402WGF1001TCE","UNI-ROYAL(厚声)","C11702","LCSC"]
["34",1,"100kΩ","R27","R0402","100kΩ","RC0402FR-07100KL","YAGEO(国巨)","C60491","LCSC"]
["35",1,"20kΩ","R28","R0402","20kΩ","0402WGF2002TCE","UNI-ROYAL(厚声)","C25765","LCSC"]
["36",2,"5.1kΩ","R50,R51","R0402","5.1kΩ","0402WGF5101TCE","UNI-ROYAL(厚声)","C25905","LCSC"]
["37",1,"120Ω","R52","R0402","120Ω","0402WGF1200TCE","UNI-ROYAL(厚声)","C25079","LCSC"]
["38",1,"TS-1185-B-A-B-A","SW1","SW-SMD_L4.0-W3.0-LS5.0","","TS-1185-B-A-B-A","XKB Connectivity(中国星坤)","C561517","LCSC"]
["39",2,"MP9943GQ-Z","U1,U2","QFN-8_L3.0-W3.0-P0.65-BL","","MP9943GQ-Z","MPS(芯源)","C477821","LCSC"]
["40",2,"MD7218E33QC3","U3,U4","SOT-23-5_L3.0-W1.7-P0.95-LS2.8-BL","","MD7218E33QC3","明达微","C920494","LCSC"]
["41",1,"ICM-42688-P","U5","LGA-14_L3.0-W2.5-P0.50-TL","","ICM-42688-P","TDK InvenSense(应美盛)","C1850418","LCSC"]
["42",1,"ICM-42605","U6","LGA-14_L3.0-W2.5-P0.50-TL","","ICM-42605","TDK InvenSense(应美盛)","C2655099","LCSC","42605的性能比42688稍差一点，也可以两个IMU都使用42688"]
["43",1,"AT7456E","U7","TSSOP-28_L9.7-W4.4-P0.65-LS6.4-BL-EP-2","","AT7456E","杭州中科微","C82351","LCSC","模拟OSD芯片，只有在玩模拟图传时需要使用，单颗价格要到15元。\n如有没有使用模拟图传的需求，可不焊接此物料！"]
["44",1,"IST8310(罗盘)","U8","LGA-16_L3.0-W3.0-P0.50-BL_SQ","","IST8310","iSentek(爱盛科技)","C2683055","LCSC","淘宝很多假货/翻新料，正常价格要7-8元/颗，如果只是玩BF固件，也可不焊接罗盘！"]
["45",2,"ZX-SH1.0-6PWT","U9,U18","CONN-SMD_6P-P1.00_MEGASTAR_ZX-SH1.0-6PWT","","ZX-SH1.0-6PWT","Megastar(兆星)","C7430448","LCSC"]
["46",1,"SPL06-001(气压计)","U10","LGA-8(2x2.5)","","SPL06-001","Goertek(歌尔)","C2684428","LCSC","V2版将气压计从DPS310，换成国产的SPL06-001。"]
["47",5,"ZX-SH1.0-4PWT","U11,U12,U14,U17,U21","CONN-SMD_4P-P1.00_MEGASTAR_ZX-SH1.0-4PWT","","ZX-SH1.0-4PWT","Megastar(兆星)","C7430446","LCSC"]
["48",2,"ZX-SH1.0-8PWT","U13,U15","CONN-SMD_8P-P1.00_MEGASTAR_ZX-SH1.0-8PWT","","ZX-SH1.0-8PWT","Megastar(兆星)","C7430450","LCSC"]
["49",1,"ZX-SH1.0-3PWT","U16","CONN-SMD_3P-P1.00_MEGASTAR_ZX-SH1.0-3PWT","","ZX-SH1.0-3PWT","Megastar(兆星)","C7430445","LCSC"]
["50",1,"TF-123-ARP9H17","U19","TF-SMD_TF-123-ARP9H15","","TF-123-ARP9H17","XUNPU(讯普)","C2982548","LCSC"]
["51",1,"TJA1051TK/3,118","U20","HVSON-8_L3.0-W3.0-P0.65-BL-EP","","TJA1051TK/3,118","NXP(恩智浦)","C124020","LCSC"]
["52",1,"GT-USB-7010ASV","USB1","USB-C-SMD_G-SWITCH_GT-USB-7010ASV","","GT-USB-7010ASV","G-Switch(品赞)","C2988369","LCSC"]
["53",1,"8MHz","X1","OSC-SMD_3P-L3.2-W1.3-P1.20-L","8MHz","CSTNE8M00GH5C000R0","muRata(村田)","C341525","LCSC"]
["54",1,"27MHz","X2","CRYSTAL-SMD_4P-L3.2-W2.5-BL_SIT8008BI","27MHz","XL2EL89COI-111YLC-27M","YXC(扬兴晶振)","C5444553","LCSC"]
[""]